
v7
1.add PIR function
2.modify record size
3.modify HTML page
3.modify record or transmit  method
4.add reset key function 

v8
1.add AP Channel selection

V9
1.add country selection
2.modify html border size
3.support special characters
4.support 2.4G
5.change PIR and rest gpio
6.change PIR strategy
7.close user-gpio

V10
1.support night vision function

V11
1.resolve no ack response problem

V12
1.add voice transmission by TCP
2.add AT command to control gpio

V13
1.Add the uplink audio support
2.Add AT command to send product ID

V14
1.support CRLF for AT command
2.change audio format from MP3 to PCM

V15
1.add RTSP audio, audio format AAC

V16
1.resolve RTSP delay or frozen problem
2.resolve RTSP can`t stream when selecting strem over wifi only mode

V17
1.add selector for RTSP selecting video and audio in html.

V18
1.resolve rstp audio reuse problem
2.delete rtsp sub channel
3.add AT command through uart2
4.add AT command "AT+AV SetVolume x" and "AT+AV SetGain"

v19
1.improve httpd priority


v21
1.resolve audio clipping when camera capture continuous dynamic scene

v22
1.Add UART Modem in html.
  two option: 
    UART2: use for uart2
    Off: receive data and transmit to TCP socket and use for AT command
2.Add AT command "AT+AV SetRecord on/off" to start and close record 

V22B
1.fix UART modem spelling mistake

V22C
1.change UART Modem
   Uart2:enabled, incoming TCP, corresponding to the Data Bypass Mode feature, will be routed to UART2
   Off: disabled

V23
1.add record on/off with AT Command when disable by html 
2.support usb ether
3.add repeater function
4.add static IP setting function

v24
1.set ntpd USA server and set PST8PDT time zone

v25
1.add Gateway and Netmask setting
2.resolve the html response delay problem

v26
1.add repeater fuction and configure automatically
2.resolve reboot crash problem in repeater mode
3.use WFV3918_HWv4_SDD(set SMPS in the SDD file to 1.8V)
4.resolve wfv3918 can`t connect router without password

V27
1.add timezone
2.set MCS 0-2 for remote
3.open usb ether
4.resolve RTSP crash problem

V28
1.add OSD function
2.add password for RTSP

V29
1.Add time zones for around the world, list US and Inida separately.
2.The name of device on router is "AmpedRF WFV3918".
3.Implement the function of Repeater.
4.Web page adjustments:
	4.1 Status View:
		4.1.1 the "SSID" , "Passwrod", "IP Address" show the actually strings when "Wifi Mode=AP"
		4.1.2 the "Band" , "Country", "IP AP Channel" show "--" when "Wifi Mode=Station"
	4.2 Wifi Configure:
		4.2.1 When "AP" selected, "SSID","Password","DHCP ", and "Gateway" can't operate.
		4.2.2 When "AP" selected, "IP Addr" and "Netmask " can be configured efficiently.
		4.2.3 When "Station" or "Repeater" selected, "Band","Country",and "AP Channel " can't operate.