###Project Name
project name = Cloud39ev200

###Devie Number
device channel = 1

###planform name
planform name = LINUX

###COM
com bOpen = 0
com base = 1
com count = 1
com baud rate = 38400

path producer = producer_39xx.bin
path nandboot = u-boot.bin

producer run addr = 0x80000000

chip type = AK_39XX_H240
chip uboot = 1
chip clock = 400
chip power off gpio = 255
chip usb2 = 1
chip pll_frep_change = 0
chip mode = 1
chip update = 0
chip test ram = 0
chip updateself = 0
chip udisk update = 0
chip select number = 1
chip select nand2 = 254
chip select nand3 = 254
chip select gpio = 0
chip gpio_pin = 254

wait time = 60
USB PID = e101
USB VID = 04d6
burned mode = 1
burned gpio = 1, 254, 1, 0, 255
burned rtc = 1, 1

cmdline support = 0
cmdline address = 0x0
cmdline data = 

ram type = 3
ram size = 64
ram row = 13
ram column = 10
ram bank = 4

mac start high = 02:02:03
mac start low = 00:00:00
mac end high = 02:02:03
mac end low = FF:FF:FF
mac addr flag = 0
fore write mac addr = 0

serial start num = AABBCCXXDDEEFFGGHH11223344556677
serial addr flag = 0
fore write serial addr = 0
BT_addr_flag = 0
fore_write_BT_addr = 0
blue_start_addr = 44A6E6000000
blue_end_addr = 44A6E6FFFFFF

auto burn flag = 1
online make image = 0
channels no fixed = 1
udisk_burn_massboot = 0
erase_partition_size_flag = 1
no_need_erase_flag = 0

moduleburn DownloadMode = 0
moduleburn bDownloadFLS = 1
moduleburn bDownloadEEP = 1
moduleburn baudrate = 921600
moduleburn gpio_dtr = 85
moduleburn gpio_module_igt = 109
moduleburn gpio_module_reset = 87
moduleburn path_fls = LCG2.fls
moduleburn path_eep = LCG2.eep

fs reserver block = 64
fs nonfs reserve size = 4

partition count = 6
	partition1 = KERNEL, 1, 1, 0, 2048
	partition2 = MAC, 0, 1, 0, 4
	partition3 = ENV, 0, 1, 0, 4
	partition4 = A, 2, 1, 0, 1024
	partition5 = B, 2, 1, 0, 4096
	partition6 = C, 2, 1, 0, 700

download_to_udisk count = 0

download_to_nand count = 1
download_to_nand1 = 1, uImage, 0x81808000, KERNEL, 0

download_to_mtd count = 3
download_to_mtd1 = 1, root.sqsh4, A
download_to_mtd2 = 1, usr.sqsh4, B
download_to_mtd3 = 1, usr.jffs2, C

download_to_spi_img count = 0

nand supported count = 0

spinand supported count = 0

sflash supported count = 14
sflash 1 = 0x1640ef, 4194304,  256, 256, 4096, 25000000, 0xf8, 0x0, w25q32, 0x0
sflash 2 = 0x1640c8, 4194304,  256, 256, 4096, 25000000, 0x0, 0x0, gd25q32, 0x0
sflash 3 = 0x1530ef, 1048576,  256, 256, 4096, 25000000, 0x0, 0x0, w25x16, 0x0
sflash 4 = 0x1540c8, 1048576,  256, 256, 4096, 25000000, 0x0, 0x0, gd25q16, 0x0
sflash 5 = 0x1440ef, 1048576,  256, 256, 4096, 25000000, 0x0, 0x0, dddddd, 0x0
sflash 6 = 0x1630ef, 4194304,  256, 256, 4096, 25000000, 0x0, 0x0, w25x32, 0x0
sflash 7 = 0x1740ef, 8388608,  256, 256, 4096, 25000000, 0x0, 0x0, w25q64, 0x0
sflash 8 = 0x1740c8, 8388608,  256, 256, 4096, 40000000, 0xf8, 0x0, gd25q64, 0x0
sflash 9 = 0x1840c8, 16777216,  256, 256, 4096, 25000000, 0xf8, 0x0, gd25q128, 0x0
sflash10 = 0x1720c2, 8388608,  256, 256, 4096, 25000000, 0x20, 0x0, mx25l6405d, 0x0
sflash11 = 0x1820c2, 16777216,  256, 256, 4096, 25000000, 0x50, 0x0, mx25l12805d, 0x0
sflash12 = 0x1840ef, 16777216,  256, 256, 4096, 25000000, 0xf8, 0x0, w25q128, 0x0
sflash13 = 0x187020, 16777216,  256, 256, 4096, 25000000, 0xf8, 0x0, xt25f128a, 0x0
sflash14 = 0x17701c, 8388608,  256, 256, 4096, 25000000, 0xf8, 0x0, PN26f64B, 0x0
