Build Version: 140711E

abSerial: 1.7

Configure Vars: 1.7

Modules: BT43H, BT24H

**Classic Profiles**

* SPP: default configuration enabled
* IAP: default configuration disabled

**BLE Profiles (BT43H only)**

* BLE GATT
* Battery Profile: default configuration enabled
* Private Service: default configuration enabled

**Enhancements**

* Added support Private BLE service

Number of characteristics is configurable from 1-10

The Service UUID is configurable

All characteristics are read/write

* Changes for Apple IAP discovery

**Known Issues**

* High speed data during 2-way exchanges may cause the module to fail. A reset is then required to continue operation
* A patch has been added to improve most cases of the above issue